Multi Power
MPW 294
INPUT		
Rated power	from 42 to 294 kW VA	
Frequency tolerance	40 to 72	
Power factor	1	
Current distorsion	< 3,5	
Voltage Range	240 to 480	
BY PASS		
Rated voltage	380-400-415 Vac, three-phase + N	
OUTPUT and INVERTER OUTPUT		
Rated power	294 kW VA	
Active power	294 kW W	
Number phases	3	
Output Voltage	380/400/415 Vac, three-phase + N 	
Dynamic stability	EN 62040-3 class performance 1 distorting load	
Frequency	50 or 60	
Load power factor	1	
ENVIRONMENTAL		
Color	RAL 9005	
Safety compliance	IEC EN 62040-1	
EMC conformance	IEC EN 62040-2 category C2	
Protection rating	IP 20 finger proof (either with cabinet doors open or close)	
Noise	< 68	
DATA		
Weight	300 Kg	
Dimensions (h w d)	610x1046x2000 mm	
Input phases	3	
Output phases	3