Multi Guard Industrial
GMI 160
INPUT		
Frequency tolerance	between 40 Hz and 72 Hz	
Power factor	>0.99	
BY PASS		
Rated voltage	220-230-240 Vac, single-phase + N	
OUTPUT and INVERTER OUTPUT		
Rated power	20000 VA	
Active power	18000 W	
Frequency	50 Hz / 60 Hz	
ENVIRONMENTAL		
Noise	from ≤ 52 dBA to ≤ 70 dBA	
DATA		
Dimensions (h w d)	745 x 620 x 320 mm