Multi Sentry
MST 100
INPUT		
Rated power	100000 VA	
Voltage	400 Vac three-phase + N Vac	
Voltage tolerance	± 20%	
Frequency tolerance	40/72 Hz	
Power factor	0.99	
BY PASS		
Rated voltage	400	
Voltage tolerance	± 15% (selectable from ± 5% to ± 25%)	
Rated frequency	50/60 Hz	
Frequency tolerance	± 5% (selectable from ± 0.25% to ± 10%)	
Number phases	3	
OUTPUT and INVERTER OUTPUT		
Rated power	100000 VA	
Active power	90000 W	
Output current	145 A	
Number phases	3	
Crest factor (Ipeak/Irms)	3 : 1	
Waveform	Sinewave	
Static stability	± 1%	
Dynamic stability	± 3% in 10 ms	
Frequency	50/60 Hz selectable	
Voltage distortion with distorcing load	3%	
Voltage distortion with linear load	1%	
Overload	125% 150% 168% of the rated current for 10' / 1' / 5	
BATTERIES		
Type	Maintenance-free sealed lead acid	
Typical recharge time	6 h 	
ENVIRONMENTAL		
Color	Dark grey RAL 7016	
Remote controls	EPO and bypass	
Communication	Double RS232/C , slot for SNMP adapter and slot for voltage free contacts.	
Safety compliance	EN 62040-1	
EMC conformance	EN 62040-2 Lev.A and Directive 73/23 EEC, 93/68 EEC, 89/336 EEC	
Protection rating	3	
AC/AC efficiency	>95% 	
Line-Interactive/Smart Active efficiency	>98%	
Noise	<56 dBA at 1 m	
Remote signals	voltage free contacts	
Operating temperature	0 ÷ 40 °C	
Relative humidity	95% no condensing	
DATA		
Weight	220 Kg	
Dimensions (h w d)	1600x500x850 mm	
Back up time	0 min