Multi Guard
GMT 120
INPUT		
Frequency tolerance	between 40 Hz and 70 Hz	
Power factor	>0.99	
BY PASS		
Rated voltage	380-400-415 Vac, three-phase + N	
OUTPUT and INVERTER OUTPUT		
Rated power	15 kVA / 13.5 kW per  module VA	
Frequency	50 Hz / 60 Hz	
ENVIRONMENTAL		
Safety compliance	IEC 62040-1	
Noise	from ≤ 60 dBA to ≤ 62 dBA